|  |  |  |  |
| --- | --- | --- | --- |
| **JOB SAFETY ANALYSIS** | **Job Task:** **Earplug Fitting Instructions****(This JSA is brand specific to those provided to White Twp)** | **Date:****2011** | **Analysis Performed By:**White Township |
| **SEQUENCE OF BASIC JOB STEPS** | **POTENTIAL HAZARDS** | **RECOMMENDED ACTION/PROCEDURE** |
| 1. Open earplugs from packaging.  | Hearing Loss due to High Noise Decibals | If reusing a set of earplugs, inspect for dirt, tears or cracks under any of three flanges. If damaged, acquire new set. |
| 2. Insert rounded tip into ear canal while pulling ear outward and upward with opposite hand.Repeat for 2nd ear. |  |  |
| 3. Check fit after inserting earplug. |  | Adjust slightly for greatest noise reduction. |
| 4. Pull earplug stem gently. Earplug should not come out of ear easily.  |  | If earplug comes out easily, completely remove earplug and repeat fitting. |
| 5. Listen to steady loud noise with earplugs in both ears. Cover ears with tightly cupped hands. Noise should sound the same whether or not ears are covered.  |  |  |
| 6. To remove earplugs. |  | Pull earplug slowly with a twisting motion to gradually break the seal. |
| 7. Once removed, inspect for dirt, tears or cracks under any of the three flanges. |  | If damaged, discard earplugs. If planning to reuse, wash with a mild soap and warm water. |