|  |  |  |  |
| --- | --- | --- | --- |
| **JOB SAFETY ANALYSIS** | **Job Task: How to safely remove Catch Basin Grate with Back Hoe** | **Date: June/2012** | **Analysis Performed By:**White Township |
| **SEQUENCE OF BASIC JOB STEPS** | **POTENTIAL HAZARDS** | **RECOMMENDED ACTION/PROCEDURE** |
| 1. Put on appropriate protective equipment. You should wear gloves, ear protection and safety glasses. | Getting hit by grate | Wear recommended equipment |
| 2. Attach chain from backhoe bucket to center of catch basin grate. Make sure chain is secure. | Grate falls | Make sure chain is secure |
| 3. Stand clear of catch basin while backhoe operator slowly lifts grate and places off to side on the ground. | Grate falls | Stay clear |
|  |  |  |