|  |  |  |  |
| --- | --- | --- | --- |
| **JOB SAFETY ANALYSIS** | **Job Task: Temporary Pot Hole Patching** | **Date: 5/2012** | **Analysis Performed By:**  Titusville – JJC –Fire Chief |
| **SEQUENCE OF BASIC JOB STEPS** | **POTENTIAL HAZARDS** | **RECOMMENDED ACTION/PROCEDURE** | |
| 1. Project & job site overview | Personal injury | Ensure a complete jobsite overview including traffic flow and all hazards  PPE – hard hat, hi-viz vest, safety glasses, steel toe boots, gloves | |
| 2. Set up appropriate signs & traffic control | Slip & fall  Injury to back, shoulder, or arm  Cuts & pinches to hands and feet  Hit by object | Use proper lifting techniques  Use appropriate PPE  Be aware of footing  Ensure a safe path in work area | |
| 3. Place equipment on road | Injuries or collisions | Wear PPE  Use traffic warning devices | |
| 4.Prep pot hole | Slip & fall  Injury to back, shoulder, or arm | Use proper lifting techniques  Ensure clear path to & from equipment | |
| 5.Back truck to pot hole | Equipment damages & personal injury | Use a back up person & follow SOP | |
| 6.Apply materials | Slip & fall  Injury to back, shoulder, or arm  Foot injury | Ensure clear path  Use proper PPE | |
| 7.Level & compact materials | Personal injury  Foot injury  Traffic hazards | Stay in work zone  Wear proper PPE  Keep equipment clean, avoid asphalt build up | |
| 8.Clean up work area | Slip & fall  Traffic hazards | Ensure clear pathway  Clear work zone safely | |
| 9. |  |  | |