|  |  |  |  |
| --- | --- | --- | --- |
| **JOB SAFETY ANALYSIS** | **Job Task: Temporary Pot Hole Patching**  | **Date: 5/2012** | **Analysis Performed By:**Titusville – JJC –Fire Chief  |
| **SEQUENCE OF BASIC JOB STEPS** | **POTENTIAL HAZARDS** | **RECOMMENDED ACTION/PROCEDURE** |
| 1. Project & job site overview  | Personal injury  | Ensure a complete jobsite overview including traffic flow and all hazardsPPE – hard hat, hi-viz vest, safety glasses, steel toe boots, gloves |
| 2. Set up appropriate signs & traffic control | Slip & fallInjury to back, shoulder, or armCuts & pinches to hands and feetHit by object  | Use proper lifting techniquesUse appropriate PPEBe aware of footingEnsure a safe path in work area |
| 3. Place equipment on road | Injuries or collisions | Wear PPEUse traffic warning devices |
| 4.Prep pot hole   | Slip & fallInjury to back, shoulder, or arm | Use proper lifting techniquesEnsure clear path to & from equipment  |
| 5.Back truck to pot hole  | Equipment damages & personal injury | Use a back up person & follow SOP |
| 6.Apply materials  | Slip & fallInjury to back, shoulder, or arm Foot injury  | Ensure clear path Use proper PPE  |
| 7.Level & compact materials  | Personal injuryFoot injuryTraffic hazards | Stay in work zoneWear proper PPEKeep equipment clean, avoid asphalt build up  |
| 8.Clean up work area  | Slip & fallTraffic hazards  | Ensure clear pathwayClear work zone safely  |
| 9. |  |  |