|  |  |  |  |
| --- | --- | --- | --- |
| **JOB SAFETY ANALYSIS** | **Job Task: How to safely Clear Sewer Rights of Way using a machete** | **Date: June/2012** | **Analysis Performed By:**  White Township |
| **SEQUENCE OF BASIC JOB STEPS** | **POTENTIAL HAZARDS** | **RECOMMENDED ACTION/PROCEDURE** | |
| 1. Put on appropriate gloves, eye protection, hard hat and leg guards. | Cutting yourself | Wear appropriate equipment | |
| 2. Make sure you have good footing and always swing machete in a forward motion and not across the body. | Cutting yourself | Follow basic job step | |
| 3. Keep your other hand close to your body. | Cutting yourself | Keep other hand close to body | |
| 4. Take small steps, do not take large, lunging steps forward. | Falling, Cutting yourself | Follow basic job step | |